Lab 3: Aluminum cantilever with strain gauges

Parts list:

Aluminum bar (~2 mm x 10 mm x 15 mm, not critical)

C-clamps to mount the free end of the cantilever to a table

Pre-wired Strain GagesS, Item# KFH-03-120-C1-11L1M2R (pack of 10), 2 leads

<https://www.omega.com/en-us/sensors-and-sensing-equipment/pressure-and-strain/strain-gauges/p/KFH>

